{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["драга 250, 210","драга 380","экскаватор","бульдозер","дробилка"],"not_rendered":{"charts":0,"images":196,"macros":1,"external_links":0,"defined_names":0,"comments":5,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"драга 250, 210","index":0,"n_rows":114,"n_cols":9,"rows_kept":114,"cut":false,"hidden":false,"merged":[[1,0,1,5],[0,0,0,5]]}
["КАТАЛОГ"]
["НА ЗАПАСНЫЕ ЧАСТИ  К ДРАГЕ  250 л., 210 л."]
[]
["К/карта","№ чертежа","Наименование изделий","Чистый вес (кг)","Марка стали","изображение",null,"Цена на 01.02.2011","Цена без НДС"]
[" ",null,"Цепь черпаковая"]
[null,null,"Наделка к черпаку",60,"Г-13"]
[null,null,"Наделка к черпаку",108,"Г-13"]
[null,52999,"Полувтулка черпака",6.5,"Г-13",null,null,{"$f":"F6","v":0},{"$f":"F6/1.18","v":0}]
[8476,52383,"Палец черпака - ремонт",88,"37ХНЗА",null,null,0,{"$f":"F7/1.18","v":0}]
[null,null,"Черпаковая рама",null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[8536,"250Д2-Р-Г","Подчерпаковый ролик",597,"сб.",null,null,{"$f":"F8","v":0},{"$f":"F8/1.18","v":0}]
[5833,"250Д2-Р-1","Стойка",61,"ст. 35Л",null,null,{"$f":"F9","v":0},{"$f":"F9/1.18","v":0}]
[10737,"210Д2-16/1","Крышка торцевая",148,"ст. 35Л",null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[4670,"А210Д2-18/1","Вкладыш",183,"бронза",null,null,null,{"$f":"F10/1.18","v":0}]
[null,"А210Д2-18/1","Вкладыш",183,"С4 24-44",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[4356,"210Д2-18/2","Шайба",49,"ст. 40",null,52273,66699.55,{"$f":"F11/1.18","v":0}]
[5077,"210Д2-18/3","Шайба",33,"ст. 35 ",null,8625,12128.79,0]
[7233,"210Д2-19/2","Втулка",17.5,"ст. 40",null,null,null,0]
[6612,"210Д2-19/4","Стяжной болт",84.3,"ст. 5",null,50581,122758.39,0]
[6613,"210Д2-19/3","Гайка М 76",3.8,"ст. 3",null,22552.880000000001,35781.31,0]
[5891,"210Д2-19/5","Шайба",35,"ст.3",null,null,null,0]
["2620/1","210Д2-28/1","Уплотнение",3,"резина",null,null,null,0]
[2620,"210Д2-28/3","Уплотнение",0.26,"резина",null,4559.2299999999996,6106.55,0]
[null,null,"Лебёдки",null,null,null,9476.6,11990,0]
[2160,"Н0Р42-216","Муфта зубчатая",49.3,"сб.",null,694,903.43,0]
[5497,"210Д6-4А","Муфта тормозная",71.400000000000006,"сб.",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[794,"210Д6-10/1А","Зубчатое колесо",246.4,"40Х",null,null,null,{"$f":"F21/1.18","v":0}]
[6619,"210Д6-21/3","Канатный ролик",40,35,null,1419,2457.4,{"$f":"F22/1.18","v":0}]
[6620,"210Д6-22/1","Втулка",2.2999999999999998,"чугун",null,284.69100000000003,524.26,{"$f":"F23/1.18","v":0}]
[7508,"210Д6-20","Ролик поддерживающий",35.5,"ст. 5",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,null,"Бегущий такелаж",null,null,null,null,null,{"$f":"F24/1.18","v":0}]
[10164,"210Д10-29А","Береговой ролик",325,"сб.",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[10166,"210Д10-30/2","Блок",56,"35Л-1",null,null,null,{"$f":"F25/1.18","v":0}]
[10171,"210Д10-20/1","Скоба",13.2,"35Х",null,null,null,0]
[7134,"210Д10-16/2","Блок",84.6,35,null,39595.047195000006,77974.05,0]
[null,null,"Главный привод",null,null,null,null,null,0]
[null,"КН - 01","Накладка на каблук",115,"Г - 13",null,null,null,0]
[null,"210Д4-16/2","Накладка на зуб",60,"Г - 13",null,null,null,0]
[null,"210Д4-16/3","Накладка на грань",36,"Г - 13",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"210Д4-16/4","Накладка на ухо",12,"Г - 13",null,null,null,{"$f":"F31/1.18","v":0}]
[4819,"250Д4-70/3","Вкладыш   ",0.21,"резина",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[1841,"210Д4-17/1","Винт М 36 Х 170",1.7,"ст. 35",null,null,null,{"$f":"F32/1.18","v":0}]
[null,"210Д4-17/1","Винт М 36 Х 225",2,"ст. 35",null,6854.0084580000012,13877.5,{"$f":"F33/1.18","v":0}]
[null,"б/ч.","Гайка М 36",0.5,"ст.  3",null,904.81380000000001,2378.17,{"$f":"F34/1.18","v":0}]
[null,null,"Бочка драги 250 л.",null,null,null,7346.4877750000005,15263.01,{"$f":"F35/1.18","v":0}]
[null,"250Д12-3/20Н","Лист перфорированный",null,"Г - 13",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"250Д12-3/21Н","Лист перфорированный",null,"Г - 13",null,null,null,{"$f":"F36/1.18","v":0}]
[null,"250Д13-3/22Н","Лист перфорированный",null,"Г - 13",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"250Д12-2/1Н","Лист перфорированный",null,"Г - 13",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"250Д12-3/14Н","Лист перфорированный",null,"Г - 13",null,null,{"$f":"F37","v":0},{"$f":"F37/1.18","v":0}]
[null,"250Д12-3/15Н","Лист перфорированный",null,"Г - 13",null,null,{"$f":"F38","v":0},0]
[null,"250Д12-63/1Н","Наборина",null,"Г - 13",null,null,{"$f":"F39","v":0},0]
[null,null,"Привод бочки драги 250 л.",null,null,null,null,{"$f":"F40","v":0},0]
[10158,"250Д13-3/А","Ролик поддерживающий",1137.9000000000001,"сб.",null,285.79232000000007,538.67999999999995,0]
[5242,"250д13-216","Направляющий ролик",320,"сб.",null,230.90100000000001,679.56,0]
[4762,"250д13-17/А/3","Корпус направляющего ролика",120,"сб.",null,274.29913500000004,857.79,0]
[4750,"250Д13-217","Упорный ролик",554.4,"сб.",null,86.68,160.88,0]
[4761,"250Д13-17/А/2А","Корпус упорного ролика",200,"ст. 35",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[7047,"63-41-2/00","Муфта в сборе",592.5,"сб."]
[null,"250Д12-63/1А","Наборина",30,"Г - 13",null,null,null,{"$f":"F45/1.18","v":0}]
[null,null,"Бочка драги 210 л.",null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"210Д12-7/11","Лист перфорированный Ф10",null,"Г - 13",null,null,null,{"$f":"F46/1.18","v":0}]
[null,"210Д12-7/12","Лист сеющий Ф12",null,"Г - 13",null,null,null,0]
[null,"210Д12-7/13","Лист сеющий Ф14",null,"Г - 13",null,null,null,0]
[null,"210Д12-7/14","Лист сеющий Ф16",null,"Г - 13",null,null,null,0]
[null,"210Д12-7/15","Лист перфорированный Ф25",null,"Г - 13",null,null,null,0]
[null,"210Д12-2/3А","Наборина",null,"Г - 13",null,null,null,0]
[null,"69Д12-06","Порог",49,"Г - 13",null,null,null,0]
[null,null,"Привод бочки драги 210л.",null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[5736,"210Д13-2","Ведущий ролик",1129.2,"сб.",null,null,null,{"$f":"F53/1.18","v":0}]
[7061,"210Д13-3/А","Поддерживающий ролик",551.29999999999995,"сб.",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[5201,"210Д13-5А","Направляющий ролик",137,"сб.",null,77986.750600000014,156917.72,{"$f":"F54/1.18","v":0}]
[6937,"210Д13-5/Б","Упорный ролик",220.5,"6155-85",null,23132.78,50611.23,{"$f":"F55/1.18","v":0}]
[588,"42-6А","Зубчатая муфта",75.2,"сб.",null,11302.852000000001,24105.439999999999,{"$f":"F56/1.18","v":0}]
[null,null,"Главный транспортер",null,null,null,29428.41,78818.679999999993,{"$f":"F57/1.18","v":0}]
[10003,"250Д15-100","Стойка крайняя",6,"ст. 35Л",null,15987.972000000002,33041.800000000003,{"$f":"F58/1.18","v":0}]
[10002,"250Д15-101/1","Стойка средняя",2.6,"ст. 35Л",null,null,161198.95000000001,{"$f":"F60/1.18","v":0}]
[null,null,"Подвес черпаковой рамы",null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[6610,"210ДЗ-11/1","Блок Ф 900",152,"ст.35",null,null,null,{"$f":"F61/1.18","v":0}]
[6611,"210ДЗ-36","Блок нижнего полиспаста",202,"ст.35Л",null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
["6611/1","210ДЗ-8/9","Втулка",4.5,"бронза",null,null,null,{"$f":"F62/1.18","v":0}]
[2007,"210ДЗ-24/1","Уплотнение",0.4,"резина",null,null,null,0]
["2007/1","210ДЗ-24/2","Уплотнение",0.04,"резина",null,null,null,0]
[1460,"250ДЗ-25","Манжета",0.68,"резина",null,null,null,0]
[723,"250Д5-11/1","Полумуфта",46,"35Л",null,null,null,0]
[751,"250Д5-11/2","Шкив тормозной",87,"чугун",null,null,null,0]
[null,null,"Драга 135 (Высочайший)",null,null,null,null,null,0]
[null,null,"Бочка"]
[null,"135.621.1","Наборина",null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,"135.621.5","Накладка каблучная",190,"Г - 13"]
[null,"135.621.3","Накладка",37,"Г - 13",null,null,null,{"$f":"F69/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,{"$f":"F70/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"F71/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"F72/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"F73/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"F74/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,{"$f":"F75/1.18","v":0}]
[null,null,null,null,null,null,892.3818340800002,2639.35,{"$f":"F76/1.18","v":0}]
[null,null,null,null,null,null,998.66800000000012,1890.5,{"$f":"F77/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,{"$f":"F78/1.18","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"#REF!/1.18","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,28128.66,{"$f":"F79/1.18","v":0}]
[null,null,null,null,null,null,null,24151.51,0]
[null,null,null,null,null,null,null,3602.4,0]
[null,null,null,null,null,null,null,810.49,0]
[null,null,null,null,null,null,null,154.66,0]
[null,null,null,null,null,null,null,1244.94,0]
[null,null,null,null,null,null,null,12399.06,0]
[null,null,null,null,null,null,null,18127.77,0]
[null,null,null,null,null,null,null,null,0]
[null,null,null,null,null,null,null,null,{"$f":"F89/1.18","v":0}]

{"sheet":"драга 380","index":1,"n_rows":140,"n_cols":6,"rows_kept":140,"cut":false,"hidden":false,"merged":[[1,0,1,5],[0,0,0,5]]}
["КАТАЛОГ"]
["НА ЗАПАСНЫЕ ЧАСТИ  К ДРАГЕ 380 л."]
[]
["К/карта","№ чертежа","Наименование изделий","Чистый вес (кг)","Марка стали","изображение"]
[null,null,"Черпаковая цепь"]
[6418,"17-76-0","Черпак - ремонт",1796,"Г-13"]
[null,null,"Наделка к черпаку",82,"Г-13"]
[null,null,"Наделка к черпаку",120,"Г-13"]
[null,"6-12А","Полувтулка черпака",16,"Г-13"]
[6417,"4/12 .","Палец черпака - ремонт",200,"37ХН3А"]
[null,null,"Черпаковая рама"]
[8536,"11/1С","Подчерпаковый ролик в сборе",713.4,"сб."]
[1924,"А15-11","Стойка",73,"35 Л "]
[1923,"112-ОА/2Г","Букса",98,"сб."]
[1922,"112-ОА/1","Втулка",44.3,"сч.15-32"]
["1924а","9/11.","Уплотнительное кольцо",0.95,"резина"]
[4288,"38-01-ООА","Защитный брус",420,"35Л"]
[null,null,"Подвес черпаковой рамы"]
[10446,"3/13-2","Ось нижних полиспастов",805,"40Х"]
[1378,"10/13-2","Уплотнение",0.66,"резина"]
[null,null,"Главный привод"]
[null,"21563-Д7","Накладка на зуб",190,"Г-13"]
[null,"5/150-1-1","Накладка на грань",60,"Г-13"]
[null,"2/15-1-1","Накладка на ухо",12,"Г-13"]
[5446,"72-9-1А","Полумуфта",19.7,"СТ40"]
[5446,"72-10-2А","Полумуфта",19.3,"СТ40"]
["5445/1","6/34-5 2/34-5  ","Втулка муфты",27.9,"СТ40"]
[5448,"72-11-12","Крышка",6.1,"СТ-40"]
[2572,"9/15-1-1","Болт М 42 Z=210",2.5,"ст. 40"]
[2572,"8/15-1-1","Болт М 42 Z=240",2.8,"ст. 40"]
[2572,"6/15-1-1","Болт М 42 Z=250",2.9,"ст. 40"]
[2572,"7/15-1-1","Болт М 42Z=270",3,"ст. 40"]
[null,"б/ч","Гайка М 42",0.62,"ст. 3"]
[9202,"11/15.","Шпилька М 48 Z=1100",15.63,"ст. 40"]
[null,"11/15.","Шпилька М 48 Z=1200",17.05,"ст. 40"]
[null,"11/15.","Шпилька М 48 Z=1600",22.79,"ст. 40"]
[null,"11/15.","Шпилька М 48 Z=1800",25.57,"ст. 40"]
[null,"б/ч","Гайка М 48",1,"ст. 3"]
[4465,"15-003Р-18А-4","Вкладыш   ",1.67,"резина"]
["71/1","14/15.","Малая шестерня",670,"36НГВ"]
[null,null,"НЧБ "]
[4672,"2/08-2","Полувтулка",260,"бронза"]
[4672,"2/08-2","Полувтулка",260,"чугун"]
[7894,"8/08-2.","Стакан",29.3,"ст. 45"]
[6766,"9/08-2.","Стержень стяжной",128,"ст. 25"]
[6767,"16/08-2.","Гайка специальная",7.74,"ст. 45"]
[7226,"11/08-2.","Кольцо сферическое",28,"ст. 45"]
[7227,"12/08-2.","Кольцо сферическое",25,"ст. 45"]
[7228,"13/08-2.","Кольцо  ",31,"ст. 45"]
[7229,"14/08-2.","Кольцо",5.4,"ст. 40"]
[7231,"18/08-2А","Крышка",120,"ст. Л36-1"]
[860,"24/08-2.","Уплотнение",7.1,"резина"]
[9906,"21523-31Б","Вкладыш НЧБ",540,"бронза"]
[null,"21523-31Б","Вкладыш НЧБ",540,"чугун"]
[null,null,"Главный транспортер"]
[9073,"24-80-1А","Верхний ролик  стакера без подш. и трубы",22.6,"сб."]
[null,"24-90-1А","Нижний ролик стакера",52,"сб."]
[9077,"3-14-29/1А","Втулка",3.68,"ст. 3"]
[9078,"5/24-8С","Крышка",0.16,"ст. 3"]
[9079,"9/24-8А","Корпус уплотнительного кольца",0.53,"ст. 25"]
[5975,"13А/24-80","Кольцо",2E-3,"резина"]
[null,"14А/24-80","Кольцо",2E-3,"резина"]
[5976,"24-90-А5","Манжета",1.6E-2,"резина"]
["5976/1","24-8-2А","Уплотнительное кольцо",0.02,"резина"]
[57,"1/24.","Кронштейн",3.1,"ст. Л36-1"]
[5126,"29/24","Кронштейн средний",4,"ст. 35"]
[5127,"30/24","Кронштейн крайний",5.8,"ст. 35"]
["724/1","20/24А","Шкив ведущий",200,"ст. 35А"]
[10295,"17/24-3А","Шестерня ведущая",37.9,"ст. 40"]
[null,null,"Свайные направляющие"]
[6768,"39-2-2","Тяга буферная",81,"ст. 35"]
[6769,"4/39-2","Гайка",3.8,"ст. 25"]
[5469,"4/39-3","Тяга буферная",50.6,"ст. 25"]
[null,"б/ч.","Гайка М 64",2.1,"ст. 3 "]
[null,"б/ч.","Гайка М 72",3.2,"ст. 3"]
[4792,"1/39-1","Корпус упора",1165,"ст.Л 36"]
[4790,"2/39-1","Полувтулка",48.4,"ст. 3"]
[4791,"3/39-1","Вкладыш",812,"ст.Л 36"]
[4794,"2/39-3","Подкладка буферная",120,"ст.Л 35-1"]
[4009,"3/39-3","Шайба направляющая",38,"ст.Л 36"]
[4795,"7/39-3","Тарелка буферная",47.8,"ст. Л 35-1"]
[4796,"8/39-3","Палец",88,"ст. 40"]
[4798,"10/39-3","Коромысло",63,"ст. 3"]
[null,null,"Лебедки маневровые  (носовые)"]
[4775,"1/34-2","Шестерня",470,"ст. 40Х"]
[7050,"2/34-2","Шестерня",270,"ст. 40Х"]
[3390,"34-3-1Д ","Шестерня",109,"ст. 35Л"]
[10960,"34-13-1","Ролик направляющий в сборе",61,"сб."]
[4377,"34-6-Б","Эластичная муфта",74.3,"сб."]
[null,null,"Бегучий такелаж"]
[4071,"36-11-20","Береговой блок в сб.",836,"сб."]
[4075,"1/36-11Б","Блок",220,"ст. 35"]
[4090,"2/36-11-2А","Втулка",7.6,"бронза"]
[4076,"2/36-11А","Уплотнение",2.2999999999999998,"резина"]
[4556,"26-00А","Передвижной такелажный блок",38,"сб."]
[4555,"26-01А","Блок",20.2,"ст.5"]
[4558,"26-07.","Подвеска блока",12,"ст. 5"]
[7286,"1/36-3-2","Блок D720",107,"ст.Л 36-1"]
[7288,"3/36-3-2","Втулка",7,"бронза"]
[2846,"2/36-3","Щека корпуса",163,"ст.л 36-1"]
[null,null,"Бочка"]
[8264,"18-2АСБ","Верхний глухой став без бандажа",6503,"сб."]
[null,"18-3АСБ","Нижний глухой став без бандажа",11017,"сб."]
[9626,"380Д18-100","Ребро (усиленное) - ремонт",2142,"сб."]
[6559,"21123Р-6А","Сменный глухой лист Z=1400",320,"Г-13"]
[null,"21123Р-6Н","Сменный глухой лист Z=1900",465,"Г-13"]
[null,"18129-В/1","Сеющий лист 1 става",330,"Г-13"]
[null,"18129-В/2","Сеющий лист 2 става",330,"Г-13"]
[null,"18129-В/3","Сеющий лист 3 става",305,"Г-13"]
[null,"18129-В/4","Сеющий лист 4 става",305,"Г-13"]
[null,"18129-В/5","Сеющий лист 5 става",305,"Г-13"]
[3477,"21123Р-41","Наружная стыковая планка",23.3,"ст. 3"]
[null,"2-18.","Наборина",18,"Г-13"]
[null,"4-18.","Порог",39,"Г-13"]
[null,"21643-29","Внутренняя стыковая планка",20,"Г-13"]
[null,"21123-36-2","Продольно-защитная накладка",36,"Г-13"]
[null,"21123-37","Продольно-защитная накладка",36,"Г-13"]
[null,"б/ч","Болт М 24 х 90 с гайкой",{"$f":"0.48+0.15","v":0.63},"ст. 3"]
[null,"б/ч ","Болт М 24 х 140 с гайкой",{"$f":"0.55+0.15","v":0.70000000000000007},"ст. 3"]
[null,"б/ч ","Гайка М 24,22 ",0.15,"ст. 3"]
[null,"б/ч ","Болт М 22 х115 с гайкой",{"$f":"0.35+0.15","v":0.5},"ст. 3"]
[null,"б/ч","Болт М 22 х 140 с гайкой",{"$f":"0.45+0.15","v":0.6},"ст. 3"]
[null,null,"Ппривод бочки"]
[6599,"4/19-0","Вал 1 передачи в сборе (без подш.)",165,"сб."]
[6749,"5/19-0","Вал 2 передачи в сборе (без подш.)",443,"сб."]
[9484,"19-6-В","Второй промежуточный вал в сб.",713,"сб."]
[1908,"19-6Г","Выходной вал",1205,"сб."]
[3951,"380Д-0000000СБ","Ведущий ролик",5000,"сб."]
[3951,"380Д-0000000СБ","Ведущий ролик без корпуса",null,"сб."]
[7054,"250Д13-3Д2","Ролик поддерживающий  без корпуса",null,"сб."]
[6547,"19-3А-1А","Ролик упорный с кронштейном",575,"сб."]
[10123,"19-3Б","Ролик направляющий",304,"сб."]
[1798,"14-21.","Полумуфта внутренняя",124,"ст. 45"]
[5495,"65-19-38","Муфта наружная",98.7,"ст. 25"]
[1839,"65-19-32","Фланец",26,"ст. 3"]
[null,null,"Ведущий ролик с валом"]
[null,null,"Ролик поддерживающий с валом"]
[null,null,"Ведущий ролик с корпусом"]
[null,null,"ВЧБ"]
[null,"21563-Д-7-А","Накладка на зуб",190,"Г-3"]

{"sheet":"экскаватор","index":2,"n_rows":87,"n_cols":7,"rows_kept":87,"cut":false,"hidden":false,"merged":[[1,0,1,5],[0,0,0,5]]}
["КАТАЛОГ"]
["на запасные части к экскаваторам"]
[]
["К/карта ","№ чертежа","Наименование изделий","Чистый вес (кг)","Марка стали","изображение","Цена на 30.12.2010 ( с НДС)"]
[null,null,"Экскаватор ЭШ - 10/60"]
[null,"1001.01.50А","Зуб ковша ",125,"Г -13"]
[null,"8/08-СБА","Козырёк",1600,"Г -13"]
[null,null,"Угольник боковой",400,"Г -13",null,{"$f":"F6","v":0}]
[null,"3-28722","Подошва",62,"Угл.",null,{"$f":"F7","v":0}]
[9958,"1-130227","Блок наводки",1250,"ст.30Л",null,{"$f":"F8","v":0}]
[7112,"2-105194А","Блок следящий",760,"ст.30Л",null,{"$f":"F9","v":0}]
[null,"2-155809А","Угольник  ",125,"ст.30Л",null,119699.98]
[null,"2-155812А","Угольник",125,"ст. 30Л",null,74468.759999999995]
[5866,"1-129463","Проушина передняя",85,"ст. 30Л"]
[6390,"2-139484","Проушина боковая",95,"ст. 30Л"]
[5568,"1-150376А","Серьга передняя",150,"ст. 30Л",null,14519.2]
[4616,"4-44661","Палец",7.5,"ст. 40Х",null,15337.2]
[8634,"4-417618","Валик",9,"40НХ",null,18653.7]
[5028,"4-41.91.97","Ось Ф 105 Х 560",38.200000000000003,"40НХ",null,1120.0999999999999]
[4499,"3-55735","Коуш подъёмный",20,"37ХНЗА",null,1375.7]
[2238,"3-55734А","Коуш тяговый",60,"37ХНЗА",null,6456.11]
[2239,"3-55748А","Коуш разгрузочный",25.3,"37ХНЗА",null,5916.6]
["3333/1","1-26239Б","Тройная проушина",178,"37ХНЗА",null,9525.2999999999993]
[5603,"К3-13-00","Концевое звено",11.38,"сб.",null,4323.3]
[null,"3-22824","Кольцо - поковка без обработки",11.5,"40Х",null,46814.97]
[null,"3-55732","Кольцо - поковка без обработки",28,"40Х",null,3995.88]
[3059,"3-30528","Ролик поворотного круга",24,"ст. 45",null,809.93]
["3059/1","3-30528Р","Ролик поворотного круга - ремонтный",30,"ст. 45",null,1972]
[5084,"3-174601","Ось  ",5,"с.ч. 15-32",null,5100]
[7285,"1-83608А","Колесо зубчатое",1324,"ст.35Л",null,5374.96]
[5385,"2-47475","Колесо зубчатое",125,"37ХНЗА",null,1727.14]
[5432,"2-47487А","Колесо зубчатое",296,"37ХНЗА",null,200633.3]
[5386,"2-47484","Вал - шестерня",122,"37ХНЗА",null,25281.599999999999]
[4452,"2-47483","Вал - шестерня",267,"37ХНЗА",null,52898.3]
[3575,"2-29122","Блок Ф600",55,"ст. 30Л",null,32440.81]
[7255,"2-56081","Тормозной шкив",190,"ст. 30Л",null,63106.87]
[4192,"2-62642","Полумуфта моторная",48.8,"ст. 30Л",null,95555.6]
[5688,"4-50473","Сектор блока наводки",12,"с.ч. 15-32",null,50493.73]
[null,null,"Экскаватор - ЭШ 20/90",null,null,null,21272.62]
[6095,"1040-61-93","Скоба с 2-мя втулками",null,null,null,2015.32]
[null,"1060.61.403","Коронка",106,"Г  -13"]
[7921,"1053.05.68СБ","Скоба с 2-мя втулками",235.1,"ст. 35Л"]
[7885,"1060.61.583","Тяга",110,"ст. 35ХНЛ"]
[8807,"1060.61.455","Проушина",180,"ст. 25Л"]
[null,"1060.61.456","Проушина",180,"ст.25Л"]
[8855,"20.90.00СБ","Звено соединительное",65.8,"сб.",null,20436.21]
[7569,"1060.61.402","Болт М 56",8.5,"ст. 40",null,9893.83]
[null,"б/ч","Гайка М 56",1.8,"ст 3",null,43745.88]
[7313,"1058.61.206","Втулка коническая",120,"35ХНЛ",null,17439.16]
[7260,"1058.61.207","Траверса",100,"ст.40Х",null,28266.55]
[8412,"1055.12.226","Ось упряжи ковша",27,"38ХГН",null,28266.55]
[8411,"1053.05.84","Ось упряжи ковша",28,"38ХГН",null,13897.61]
[8410,"1053.05.47","Ось упряжи ковша",73,"38ХГН",null,2408.84]
[8409,"1043.61.42","Ось упряжи ковша",28.4,"38ХГН",null,306.61]
[9954,"1060.61.568","Траверса",105,"ст.35ХНЛ",null,19761.32]
[10352,"1060.21.621","Втулка подъёмного цилиндра",588,"ст.35ХНЛ",null,15737.8]
[null,null,"Экскаватор ЭКГ - 4,6",null,null,null,4429.4399999999996]
[null,"1001.01.50А","Зуб ковша",125,"Г -13",null,4446.7]
[5237,"1001.38.01-1","Звено гусеничное",232,"Г -13",null,9790.26]
[5237,"1001.38.01-1","Звено гусеничное",232,"угл.",null,3509.56]
[9650,"1001.06.08.4","Колесо ведущее",585,"ст. 45",null,21933.84]
[9650,"1001.06.08.4-5","Колесо ведущее",585,"ремонт",null,117544.66]
[8242,"1080.05.307","Ползун",76,"с.ч.20"]
[8243,"1080.05.308","Ползун боковой",14.5,"с.ч.20"]
[7635,"1001.90.02","Палец звена",2.2999999999999998,"ст. 40Х"]
[null,null,"Экскаватор ЭШ 15/90",null,null,null,{"$f":"F58","v":0}]
[2387,"1004.04.01-Р","Ролик (заготовка ЭШП)",70.5,"37ХНЗ",null,{"$f":"F59","v":0}]
[6146,"1030.04.03-1","Ось ролика",18,"сч.18-36",null,28840.55]
[null,null,"Эскаватор ЭО41-21А",null,null,null,70543.34]
[8342,"ОМА-951","Зуб",11.5,"40ХН",null,43359.9]
[null,"41-21-00","Зуб",11.5,"40ХН",null,11323.68]
[null,null,"Эскаватор ЭО5124",null,null,null,3138.88]
[null,"АЛ-24","Зуб",null,"40ХН",null,701.35]
[null,null,"Эскаватор ЭО5126"]
[null,"51-26-00","Коронка",11,"Г-13"]
[null,null,"Эскаватор РС-400"]
[null,"РС-400-7/3","Коронка",15,"Г-13",null,13686.49]
[null,null,"Эскаватор Хитачи",null,null,null,4813.46]
[null,"Э.0802.152","Коронка",24,"Г-13"]
[null,null,"Эскаватор 325DL"]
[null,"325DL-466","Коронка",16,"Г-13"]
[null,null,"Эскаватор РС-220"]
[null,"РС-220-6-1","Коронка",null,null,null,1047.3800000000001]
[]
[]
[null,null,null,null,null,null,"Ленсиб"]
[null,null,null,null,null,null,"Ленсиб"]

{"sheet":"бульдозер","index":3,"n_rows":150,"n_cols":6,"rows_kept":150,"cut":false,"hidden":false,"merged":[[1,1,1,5],[0,2,0,4]]}
[null,null,"Каталог"]
[null,"НА ЗАПАСНЫЕ ЧАСТИ К БУЛЬДОЗЕРАМ И ГИДРОЭЛЕВАТОРАМ"]
[]
[]
["К/карта ","№ чертежа","Наименование изделий","Чистый вес,кг.","Марка стали","изображение"]
[null,null,"Бульдозер Т - 500"]
[null,"Т500.01.002","Нож правый",95,"Г -13Л"]
[null,"Т500.01.002","Нож левый",95,"Г -13Л"]
[null,"Т500.01.001","Нож средний",120,"Г -13Л"]
[null,"КМ-15-01","Коронка ",20,"Г -13Л"]
[8201,"403-22-12","Звёздочка",158,"ст. 45Л"]
[8902,"Т500-430-85","Рыхлитель (при налич. зав. заготовки) ",650,"40ХН"]
[null,"Т500-430-85РСБ","Рыхлитель - ремонт",650,"40ХН"]
[8415,"Т160-140-00","Кулак",25,"37ХНЗА"]
[8515,"Т180-130-00СБ","Хомут",3,"37ХНЗА"]
[9080,"355-21-57СБ","Каток двубортный",110.4,"сб."]
[null,"355-21-58СБ","Каток однобортный",95,"сб."]
[8783,"Т101.00.00","Уплотнение в сборе",null,"сб."]
[9321,"Т-500-01","Болт",1.3,"ст. 40Х"]
[null,"Т-500-02","Гайка",0.6,"ст. 3"]
[351,null,"Шлифовка коленчатого вала в размер",150]
[351,null,"Шлифовка коленчатого вала ч/размер"]
[null,null,"Башмак - ремонт",null,"ст.33"]
[null,null,"Гусеница - ремонт(всё б/у)",null,"сб."]
[null,null,"(по согл. с зак.)"]
[null,null,"БУЛЬДОЗЕР Д 355"]
[null,"КМ-16-02","Нож угловой правый",60,"Г-13Л"]
[null,"КМ-16-02","Нож угловой левый",60,"Г-13Л"]
[null,"КМ-15-03","Нож средний",75,"Г-13Л"]
[null,"КМ-15-01","Коронка рыхлителя",20,"Г-13Л"]
[null,"КМ-15-0/А","Прожектор рыхлителя",35,"Г-13Л"]
[null,"25-30-01","Звёздочка",150,"ст.45Л"]
[null,null,"Гусеница - ремонт (по согл. с заказ-ом)  ",null,"сб."]
[null,null,"Шлифовка колен/валов в размер"]
[null,null,"Шлифовка колен/валов через размер"]
["4131/1","БК-28-90","Башмак  (при налич.спец.проката)",40.799999999999997,"ст.35Л"]
[null,"БК-28-90","Башмак - восстановление",40.799999999999997,"ст.35Л"]
[7206,"БК-86-12-01","Кулак толкающего бруса",39,"37ХНЗА"]
["8811/1","КР-21-90-00","Рыхлитель (при нал. зав. заготовки)",582,"40Х"]
[null,null,"БУЛЬДОЗЕР Д-375"]
[9864,"375-21-58АСБ","Каток однобортный в сборе",102.6,"сб."]
[null,"375-21-57СБ","Каток двубортный в сборе",111.7,"сб."]
[9881,"Д-375-05","Звёздочка",228,"ст.45Л"]
[null,"БМ-198-72/2","Нож центральный",135,"Г-13Л"]
[null,"Д375А","Коронка",27,"Г-13Л"]
[null,"БМ-198-72/5","Нож Угловой",140,"Г-13"]
[null,null,"БУЛЬДОЗЕР ДЭТ-250"]
[null,"Д359ХЛ01.00005","Нож левый",70,"Г-13Л"]
[null,"Д359ХЛ01.00005","Нож правый",70,"Г-13Л"]
[null,"Д3118.10.001","Нож средний",135,"Г-13Л"]
[null,null,"Шлифовка колен/вала в размер"]
[null,null,"Шлифовка колен/вала через размер"]
[null,null,"БУЛЬДОЗЕР Д9Н"]
[null,"А/МА-149-00М-01","Нож средний",55,"Г-13Л"]
[null,"А/МА-149-00М-04","Нож средний правый",55,"Г-13Л"]
[null,"А/МА-149-00М-02","Нож средний левый",55,"Г-13Л"]
[null,"А/МА-149-00М","Нож угловой правый",48,"Г-13Л"]
[null,"А/МА-149-00М","Нож угловой левый",48,"Г-13Л"]
[null,"КМ-10/5АМ","Коронка",19,"Г-13Л"]
[4213,"К-00-10А","Звёздочка",144,"ст.45Л"]
[null,null,"Шлифовка колен/вала в размер"]
[null,null,"Шлифовка колен/вала через размер"]
[null,null,"БУЛЬДОЗЕР Д 10Н, Д 8Н"]
[null,"КН-25-02","Коронка",25,"Г-13Л"]
[null,"КН-25-01","Коронка",17,"Г-13Л"]
[null,"Д.10.0103.166.05","Нож угловой левый",46,"Г-13Л"]
[null,"Д.10.0103.166.04","Нож угловой правый",46,"Г-13Л"]
[null,"Д.10Н-25-02","Коронка"]
[null,null,"БУЛЬДОЗЕР Т 130"]
[null,"Т130-03","Нож угловой правый",40,"Г-13Л"]
[null,"Т130-03","Нож угловой левый",40,"Г-13Л"]
[null,"Т130-04","Нож средний",65,"Г-13Л"]
[null,"Т130-10","Трак гусеничной цепи ",15,"ст..5сп."]
[null,null,"(при нал.спец.прок)"]
[null,null,"БУЛЬДОЗЕР \"КАТО\""]
[null,"К-27-00","Коронка",15,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР Т35"]
[null,"Т35-01-01","Коронка",26,"Г-13Л"]
[10036,"Т35-01-01","Звёздочка",122,"ст.45Л"]
[null,"Т35-01","Нож левый",97,"Г-13Л"]
[null,"Т34-01","Нож правый",97,"Г-13Л"]
[null,null,"РАЗНОЕ"]
[null,"155-01-01","Звёздочка бульдозера Д155",132,"ст.45Л"]
[null,"155-01-02","Звёздочка бульдозера Д155",132,"ст.45Л"]
[null,"Д395-01","Нож автогрейдера",60,"Г-13Л"]
[null,"101-45-11","Коронка бульдозера \"БЕЛАЗ\"",17,"Г-13Л"]
[1530,"ОМА-2739","Коронка КАМАЦУ 455",26,"Г-13Л"]
[null,"200-02","Зуб ЭО5022А",20,"Г-13Л"]
[null,"104-00","Зуб грейдера",10,"Г-13Л"]
[null,null,"ПОГРУЗЧИК БЕЛАЗ 7822-10"]
[null,"ОМА-2937","Коронка",24,"Г-13"]
[]
[null,"КФ-10-1","Погрузчик WA-600",15,"Г-13Л"]
[null,"АП-81-26","Погрузчик L-34",10,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР SD16"]
[null,"SD16-03","Нож угловой правый",20,"Г-13Л"]
[null,"SD16-02","Нож угловой левый",20,"Г-13Л"]
[null,"SD16-01","Нож средний",40,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР Т-11"]
[null,"Т-11-11-03","Нож угловой правый",30,"Г-13Л"]
[null,"Т-11-11-02","Нож угловой левый",30,"Г-13Л"]
[null,"Т-11-11-01","Нож средний",44,"Г-13Л"]
[null,"Б0707.161","Коронка",10,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР Д155"]
[null,"ДБ.0702.147.01","Коронка",16,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР Д6R"]
[null,"4Т-6761","Нож угловой",95,"Г-13Л"]
[null,"4Т-66-59Е","Нож центральный",48,"Г-13Л"]
[null,"D6R-04","Коронка",14,"Г-13Л"]
[null,null,"ТРАКТОР Т1101 (Севзото)"]
[null,"Т1101-К","Коронка",10,"Г-13"]
[null,null,"БУЛЬДОЗЕР Т-20"]
[null,"Т-20-К-04","Коронка",16,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР 364 Либхер"]
[null,"PR-34-606.3","Нож угловой правый",26,"Г-13Л"]
[null,"PR-34-606.3","Нож угловой левый",26,"Г-13Л"]
[null,"PR-34-606.2","Нож средний",34,"Г-13Л"]
[null,"PR-34-606.1","Нож средний",32,"Г-13Л"]
[null,null,"БУЛЬДОЗЕР 764 Либхер"]
[null,"764PR64.605.4","Зуб рыхлителя",40,"Г-13Л"]
[null,"764PR64.605.3","Нож угловой правый",80,"Г-13Л"]
[null,"764PR64.605.3","Нож угловой левый",80,"Г-13Л"]
[null,"764PR64.605.1","Нож средний",125,"Г-13Л"]
[null,"764PR64.605.2","Нож средний",102,"Г-13Л"]
[null,null,"Бульдозер Д9R (Caterpillar)"]
[null,"Т7-5702В","Нож средний"]
[null,"Д9R-01","Коронка",21,"Г-31"]
[null,null,"Бульдозер погрузчик 99.0"]
[null,"9N4552","Коронка"]
[null,null,"Бульдозер Хиттачи"]
[null,null,"Коронка"]
[null,null,"Бульдозер Д11R (Caterpillar)"]
[null,"9W6657","Нож крайний",95,"Г-3"]
[null,"9W2425","Нож крайний",null,"Г-13"]
[null,"Д11-01","Корона",45,"Г-13"]
[null,null,"Буровой станок Амуровец"]
[null,"Б2650005003","Шестерня"]
[null,"Б2670007007","Шкиф Фрикциона"]
[null,"Z20m=7 Б2650004006","Шестерня"]
[null,"2-14-06/75","Долото крестовое"]
[null,"Б2650004022","Шкив Малый"]
[null,null,"Гидроэлеватор ГЭ-170/350"]
[1225,"942Г-1/4а","Горловина ДУ170 ",125,"ст.35"]
[1225,"942Г-1/13","Вставка ДУ170",17,"ст.35"]
[1225,"1013ГБ-1/21","Камера приёмная",142,"ст.35"]
[1225,"1013ГБ-1/33","Колено двойное",54.5,"ст.35"]
[1225,"1017ГБ-1/2","Раструб Ф207/350",157,"ст.35"]
[1225,"1017ГБ-1/3","Переход Ф170/207",127,"ст.35"]
[1225,"1017ГБ-1/11,1/12","Насадка Ф 85, Ф 90","10,6; 11,8","ст.45"]
[1225,"657ГА-8/1","Кольцо",3.7,"ст.35"]

{"sheet":"дробилка","index":4,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[[1,0,1,5],[0,0,0,5]]}
["КАТАЛОГ"]
["НА ЗАПАСНЫЕ ЧАСТИ К ДРОБИЛКАМ И МЕЛЬНИЦАМ"]
[]
["К/карта ","№ чертежа","Наименование изделий","Чистый вес( кг)","Марка стали","Изображение"]
[null,null,"Дробилка СМД 109Д"]
[null,"СМД 109.00.00.04","Клин верхний правый",60,"Г-13Л"]
[null,"СМД 109.00.00.05","Клин верхний левый",60,"Г-13Л"]
[null,"168-0-2","Клин нижний правый",20,"Г-13Л"]
[null,"168-0-3","Клин нижний левый",20,"Г-13Л"]
[null,"СМД.109.00.00.03","Плита дробильная неподвиж.",400,"Г-13Л"]
[null,"48.449.020.17","Плита дробильная подвиж. ",510,"Г-13Л"]
[null,null,"Мельница МШР"]
[null,"1372.01.117-2СБ","Черпак",75,"Г-13Л"]
[null,"1374.03.301-1СБ","Футеровка №1",200,"Г-13Л"]
[null,"1362.03.304-СБ","Футеровка №4",100,"Г-13Л"]
[null,"1370.03.302-1СБ","Футеровка №5",155,"Г-13Л"]
[null,"1370.03.301-1","Футеровка №7",220,"Г-13Л"]
[null,"1362.04.301-СБ","Решётка",135,"Г-13Л"]
[null,"1362.04.303","Клин",35,"Г-13Л"]
[null,"1362.04.302-СБ","Футеровка центральная",155,"Г-13Л"]
[null,"К-17-01","Сегмент классификатора",4,"Г-13Л"]
[null,null,"Шаровая Мельница"]
[null,"МШЦ-45-03","Бронеплита торцевая",38,"Г-13Л"]
[null,"НС2-248","Бронеплита с греблями",71,"Г-13Л"]
[null,"НС2-250","Бронеплита шир 400",101,"Г-13Л"]
[null,"РК-1571","Бронеплита безболтовая",71,"Г-13Л"]
[null,"НС2-251","Бронеплита шир 400",100,"Г-13Л"]
[null,"РК-1571-1","Бронеплита торцевая",95,"Г-13Л"]
[null,"РК-1581","Клин затяжной",18,"Г-13Л"]
[null,"НС3-998","Клин неподвижный",15,"Г-13Л"]
[null,"П850-00-01","Футеровка",50,"Г-13Л"]
[null,"П900-00-02","Футеровка люка",95,"Г-13Л"]
[null,"П900-00-03","Футеровка рамки люка",95,"Г-13Л"]
[null,"МШЦ-45-03","Бронеплита торцевая",38,"Г-13Л"]
[null,"МШЦ-45-02","Бронеплита",50,"Г-13Л"]
[null,"МШЦ-45-04","Клин неподвижный",15,"Г-13Л"]
[null,"МШЦ-45-01","Бронеплита",47,"Г-13Л"]
[null,"М09021601М","Футеровка",95,"Г-13"]
[null,"М090216002М","Футеровка",86,"Г-13"]
[null,"М09021604М","Футеровка",62,"Г-13"]
[null,"М09182(3)","Футеровка",26,"Г-13"]
[null,"М091802","Футеровка",45,"Г-13"]
[null,null,"Мельница ВАГУ-2130"]
[null,"М090216002М","Футеровка"]
[null,"М4351-2-1","Футеровка"]
[null,"М09021603","Футеровка"]
[null,null,"Каскад 75х2,8 Телега загрузки"]
[null,"М43-51-601(02)","Броня торцевая",25,"Ст-35"]
[null,"М34-51-5.01(02)","Броня торцевая",63,"Ст-35"]
[null,"М43-51-3","Броня торцевая",76,"Ст-35"]